Title: est1247_parts.xlsx
Author: JimZ

PARTS LIST KIT N0. 1247 ‐ Cherokee‐D (Later Damon)
Quantity | Description | Type | Number | Details1 | Details2 | Details3 | Details4 | Comment
1 | PAPER BODY TUBE | BT‐50J | 30362 | 2.75" long | 0.950" ID | 0.976" OD | 0.013" wall | Glassine
1 | Pattern Sheet | SP‐47 | 83053 | 5.5" wide | 6.5" long | Cardstock | | Scan
1 | ENGINE HOLDER | EH‐2 | 35025 | 2.8" long | .100" wide | .025" thick | | Reg. & D
2 | CENTERING RINGS | AR‐5055 | 30166 | .977" ID | 1.27" OD | 0.25" long | BT‐50 in BT‐55 | Set of 2
1 | CENTERING RINGS | AR‐2050 | 30164 | 0.25" long | 0.737" ID | 0.949" OD | 0.106" wall | Green
1 | PAPER BODY TUBE | BT‐55 | 30382 | 18" long | 1.283" ID | 1.325" OD | 0.021" wall | Glassine
1 | Die‐Cut Balsa | *BF‐47 | 32220 | 4" wide | 9" long | 3/32" thick | | Scan
1 | LAUNCH LUG | LL‐2A | 38175 | 5/32" ID | 1/8" rod | 1.25" long | | Mylar
1 | Shock Cord | SC‐1 | 85730 | 18" long | 1/8" wide | | | Rubber
1 | Parachute | PK‐18A | 85566 | 18" dia. | 18" x 6 Shrouds | LDPE plastic | Org/Blk/Wht | Damon Logo
1 | Shroud Line | SLT‐108 | 38239 | 108" | .020" diameter | Twisted cotton | | For 18" to 24"
6 | Tape Disc | TD‐3F | 38406 | 1/2" dia. | Paper | Self‐Stick | WO/Center Hole | Set of 6
1 | PLASTIC NOSE CONE | PNC‐55AC | 71070 | 5.4" long | 1.325" dia. | .5" shoulder | White | Blow molded
1 | Decal Sheet | KD‐47 | 37045 | 4.5" wide | 6" long | Red/Blk | Waterslide | Scan
* | BALSA FIN STOCK | BFS‐30(4x9) | N/A | 4" wide | 9" long | 3/32" thick | 0.09375 |