Author: JimZ

PARTS LIST KIT N0. 1288
Quantity | | Description | Type | Number | | Details1 | Details2 | Details3 | Details4 | Comment
1 | STAGE COUPLER | JT-20C | 30254 | 0.650" ID | 0.708" OD | 0.75" long | fits BT-20 |
1 | PAPER BODY TUBE | BT-20 | 30316 | 18" long | 0.710" ID | 0.736" OD | 0.013" wall |
1 | PAPER BODY TUBE | BT-20B | 30320 | 8.65" long | 0.710" ID | 0.736" OD | 0.013" wall |
1 | SPLIT ADAPTER RING | AR-20508 | 80425 | BT-20 in BT-50 | | | |
3 | CENTERING RINGS | AR-2050 | | 3101 | BT-20 in BT-50 | | | |
1 | Pattern Sheet | SP-88 | 83229 | | | | | Scan
1 | ENGINE HOLDER | EH-2 | 3141/35025 | 2.8" long | .100" wide | .025" thick | | Reg. & D
1 | Shock Cord | | SC-1LD | 85743 | 1/8" x 24" | | | |
1 | PAPER BODY TUBE | BT-50J | 30362 | 2.75" long | 0.950" ID | 0.976" OD | 0.013" wall |
1 | PAPER BODY TUBE | BT-50W | 30372 | 9.5" long | 0.950" ID | 0.976" OD | 0.013" wall |
1 | BALSA FIN STOCK | BFS-40 | | 3172 | 1/8" thick | 3" wide | 9" long | | BF-88/32296
1 | Screw Eye | | SE-2A | 38252 | 3/4" long | | | |
1 | BALSA NOSE CONE | BNC-20A | 70224 | .813" long | .736" dia. | .25" shoulder | |
3 | DOWEL | | WD-1 | 32056 | 1/8" dia. | 18" long | | | Wood
1 | PAPER BODY TUBE | SBT-394AJ | 30449 | 1" long | 3.876" ID | 3.918" OD | 0.021" wall | Special for 1288 Starlab
1 | LAUNCH LUG | LL-2C | | 2325 | 5/32" ID | 1/8" rod | 5" long | |
1 | Parachute | | PK-12A | | 2263 | 12" dia. | | | |
1 | Shroud Line | SLT-72 | 38238 | 72" | | | |
6 | Tape Disc | | TD-3F | 38406 | 1/2" dia. | | | | 6x
1 | Embossed Panel Sheet | EW-88 | 37661 | | | | | Scan
1 | Die-Cut Card Sheet | TA-88 | 30064 | | | | | Scan
1 | Decal | | KD-88 | 37094 | | | | | Scan