Title: est2179.xlsx
Author: JimZ

PARTS LIST KIT N0. 2179 ‐ Guardian
Quantity | Description | Type | Number | Details1 | Details2 | Details3 | Details4 | Comment
1 | PAPER BODY TUBE | BT‐20J | 30326‐1 | 2.75" long | 0.710" ID | 0.736" OD | 0.013" wall | Blue
1 | ENGINE HOLDER | ? | 35021 | 2.8" long | .100" wide | .025" thick | | Thumb Saver
1 | MYLAR RETAINER RING | HR‐20 | 3340/30168 | .774" ID | .25" wide | | | Strapdown ring for EH‐2 and BT‐20J
1 | CENTERING RINGS | AR‐520 | 30162‐2 | .69" OD | .542" ID | 0.19" long | BT‐5 in BT‐20 | Green
1 | PLASTIC NOSE CONE | PNC‐50YR | 72604 | 4.1" long | .974" dia. | | BT‐50 ‐ Ogive | Pairs with PIN‐50YR
1 | NOSE CONE INSERT | PIN‐50YR | 72605 | .65" long | .5" shoulder | | | .65" exposed. .5" insert in cone.
1 | PLASTIC ADAPTER | TA‐5055(P) | 30101 | 3.6" long | 1.0" taper | .75" front | .85" back | Blow Molded
1 | PAPER BODY TUBE | BT‐50J | 30362 | 2.75" long | 0.950" ID | 0.976" OD | 0.013" wall | Glassine
1 | PAPER BODY TUBE | BT‐55? | 30381 | 11.25" long | 1.283" ID | 1.325" OD | 0.021" wall | Length verified on actual kit
2 | PAPER ADAPTER | RA‐2055 | 30125 | 0.738" ID | 1.27" OD | .05" thick | Set of 2 | One ring notched for engine hook.
1 | Laser cut balsa | BF‐2179 | 60415 | 4"wide | 12" long | .09375" thick | 3/32" thick | Scan
1 | Shock Cord | SC‐1 | 85730/38367 | 18 " long | 1/8" wide | | | Rubber
1 | LAUNCH LUG | LL‐2A | 2321/38175 | 5/32" ID | 1/8" rod | 1‐1/4" long | |
1 | Parachute | PK‐12A | 2263/85564/35815 | 12" dia. | | | | Pre‐assembled
1 | Decal | KD‐2179 | 60379 | 2" wide | 8.5" long | Blue/White | Self Stick | Scan