Title: k-33_parts.xlsx
Author: JimZ

PARTS LIST KIT N0. K‐33 ‐ Trident
Quantity | Description | Type | Number | Details1 | Details2 | Details3 | Details4 | Comment
1 | PAPER BODY TUBE | BT‐50W | 30372 | 9.5" long | 0.950" ID | 0.976" OD | 0.013" wall | Glassine
1 | PAPER BODY TUBE | BT‐50S | 30368 | 4" long | 0.950" ID | 0.976" OD | 0.013" wall | "Atomic Drive" Tube
3 | PAPER BODY TUBE | BT‐5 | 30302 | 18" long | 0.515" ID | 0.541" OD | 0.013" wall | "Supplies and Storage" Tube
1 | PAPER BODY TUBE | BT‐20J | 30326 | 2.75" long | 0.710" ID | 0.736" OD | 0.013" wall | Engine Holder Tube
1 | BALSA NOSE CONE | BNC‐50K | 70262 | 2.75" long | .976" dia. | .5" shoulder | | Main Nose Cone
1 | BALSA NOSE CONE | BNC‐50Y | 70266 | 4.375" long | .976" dia. | .375" shoulder | | "Passenger Section" Tail Cone
1 | BALSA NOSE CONE | BNC‐50J | 70256 | 1.375" long | .976" dia. | .5" shoulder | | "Atomic Drive" Nose Cone
3 | BALSA NOSE CONE | BNC‐5E | 70212 | 1.375" long | .541" dia. | .25" shoulder | | "Supplies and Storage" Nose Cone
3 | BALSA NOSE CONE | BNC‐5W | 70218 | 2.875" long | .541" dia. | .25" shoulder | | "Supplies and Storage" Tail Cone
6 | ADAPTER RING | RA‐2050 | 3110 | 0.738" ID | 0.949" OD | 0.02" thick | BT‐20 in BT‐50 |
1 | STAGE COUPLER | JT‐50C | 30260 | 0.920" ID | 0.949" OD | 1" long | fits BT‐50 |
1 | ENGINE HOLDER | EH‐2 | 3141/35025 | 2.8" long | .100" wide | .025" thick | | Reg. & D
1 | Shock Cord | SC‐1 | 85730 | 18 " long | 1/8" wide | | | Rubber
1 | Parachute | PK‐18A | 2266/85566 | 18" dia. | | | |
6 | Tape Strip | TD‐2F | 2297 | 1/4" x 3/4" | | | | 6x
1 | Screw Eye (Large) | SE‐1 | | 1" long | | | |
1 | LAUNCH LUG | LL‐2C | 2325 | 5/32" ID | 1/8" rod | 5" long | |
1 | BALSA FIN STOCK | BFS‐30L | 3170 | 3/32" thick | 3" wide | 12" long | 0.09375 |
1 | Pattern Sheet | SP‐33 | | | | | | Scan
1 | DOWEL | WD‐2C | ? | 1/12" dia. | 5" long | | | Wood
1 | Shroud Line | SLT‐108 | 38239 | 108" | | | |